**PROJECT DEVELOPMENT DELIVERY OF SPRINT-1**

|  |  |
| --- | --- |
| **TEAM ID** | PNT2022TMID43101 |
| **PROJECT NAME** | IoT BASED SMART CROP  PROTECTION SYSTEM FOR  AGRICULTURE |

**SPRINT-1**

#include <ESP8266WiFi.h>

#include <WiFiClient.h>

#include <PubSubClient.h>

#include "DHT.h"

const char\* ssid = "SMART-G"; const char\* password = "10112019";

#define DHTPIN D6

#define G D0

#define DHTTYPE DHT11

DHT dht(DHTPIN, DHTTYPE);

#define ID "3t3j6q"

#define DEVICE\_TYPE "ESP8266"

#define DEVICE\_ID "TEST"

#define TOKEN "TEST-12345"

char server[] = ID

".messaging.internetofthings.ibmcloud.com"; char publish\_Topic1[] = "iot-2/evt/Data1/fmt/json"; char publish\_Topic2[] = "iot-2/evt/Data2/fmt/json"; char publish\_Topic3[] = "iot-2/evt/Data2/fmt/json"; char publish\_Topic4[] = "iot-2/evt/Data2/fmt/json"; char authMethod[] = "use-token-auth"; char token[] = TOKEN; char clientId[] = "d:" ID ":" DEVICE\_TYPE ":" DEVICE\_ID;

WiFiClient wifiClient;

PubSubClient client(server, 1883, NULL, wifiClient);

void setup() { pinMode(D0,OUTPUT); digitalWrite(D0,HIGH); Serial.begin(115200); dht.begin(); Serial.println();

WiFi.begin(ssid, password); while (WiFi.status() != WL\_CONNECTED) { delay(500);

Serial.print(".");

}

Serial.println("");

Serial.println(WiFi.localIP());

if (!client.connected()) {

Serial.print("Reconnecting client to "); Serial.println(server);

while (!client.connect(clientId, authMethod, token)) {

Serial.print("."); delay(500);

}

Serial.println("Connected TO IBM IoT cloud!");

}

}

long previous\_message = 0; void loop() {

client.loop(); long current = millis(); if (current - previous\_message > 3000) { previous\_message = current; float hum = dht.readHumidity(); float temp = dht.readTemperature(); float MOI = map(analogRead(A0), 0, 1023, 100, 0); float bi = map(digitalRead(D1), 0, 1, 100, 0); if (isnan(hum) || isnan(temp) ){

Serial.println(F("Failed to read from DHT sensor!")); return;

}

Serial.print("Temperature: ");

Serial.print(temp);

Serial.print("°C");

Serial.print(" Humidity: ");

Serial.print(hum);

Serial.print("%");

Serial.print("SOIL MOITURE: ");

Serial.print(MOI);

Serial.print("ANIMAL AND BIRD: ");

Serial.print(bi); if(MOI<=10)

{

digitalWrite(D0,LOW); delay(100); digitalWrite(D0,HIGH);

}

else

{

digitalWrite(D0,HIGH);

}

String payload = "{\"d\":{\"Name\":\"" DEVICE\_ID "\""; payload += ",\"Temperature\":"; payload += temp; payload += "}}";

Serial.print("Sending payload: ");

Serial.println(payload);

if (client.publish(publish\_Topic1, (char\*) payload.c\_str())) {

Serial.println("Published successfully");

} else {

Serial.println("Failed");

}

String payload1 = "{\"d\":{\"Name\":\"" DEVICE\_ID

"\""; payload1 += ",\"Humidity\":"; payload1 += hum; payload1 += "}}";

Serial.print("Sending payload: ");

Serial.println(payload1);

Serial.println('\n');

if (client.publish(publish\_Topic2, (char\*) payload1.c\_str())) {

Serial.println("Published successfully");

} else {

Serial.println("Failed");

}

String payload3 = "{\"d\":{\"Name\":\"" DEVICE\_ID

"\""; payload3 += ",\"Moiture\":"; payload3 += MOI; payload3 += "}}";

Serial.print("Sending payload: ");

Serial.println(payload3);

if (client.publish(publish\_Topic3, (char\*) payload3.c\_str())) {

Serial.println("Published successfully");

} else {

Serial.println("Failed");

}

String payload4 = "{\"d\":{\"Name\":\"" DEVICE\_ID "\""; payload4 += ",\"Animal&Bird\":"; payload4 += bi; payload4 += "}}";

Serial.print("Sending payload: ");

Serial.println(payload4);

if (client.publish(publish\_Topic4, (char\*) payload4.c\_str())) {

Serial.println("Published successfully");

} else {

Serial.println("Failed");

}

}

}